{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["SpisPaneli - rysunek","Tabele pomocnicze"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"SpisPaneli - rysunek","index":0,"n_rows":22,"n_cols":14,"rows_kept":22,"cut":false,"hidden":false,"merged":[[1,12,1,13],[2,1,3,1],[1,3,1,6],[1,7,1,11],[2,3,2,5],[21,3,21,11],[17,3,17,11],[18,3,18,11],[19,3,19,11]],"flags":["formulas_cached_only"]}
[]
[null,null,null,"Części produkcyjne",null,null,null,"Sterownik PAS kompletny (zestaw serwisowy / naprawczy PAS)",{"$nulls":4},"Parametry programowe"]
[null,"lp","Pralka","wyposażenie pralki",null,null,"SAP Prettl -stare","Sterownik PAS","wkładka do IO","Część wewnętrzna pokrętła PAS","Podpora płytki serwisowej PAS","SAP (sterownik kompletny) -nowy","Średnica koła pasowego silnika","Układ programów"]
[null,null,"typ","AquaSpray","Czujnik AS","Pokrętła","-"]
[null,"[1]","[2]","[3]","[4]","[5]","[6]","[7]","[8]","[9]","[10]","[11]","[12]","[13]"]
[null,1,"PA ..60A411","-","-",1,8016925,"PA 60A411","+","+","+",8034621,19,2001]
[null,2,"PA ..60A420","+","-",1,8016926,"PA 60A420","+","+","+",8034623,19,2001]
[null,3,"PA ..60A420 AS","+","+",1,8016927,"PA 60A420 AS","+","+","+",8034625,19,2001]
[null,4,"PA ..80A510","-","-",1,8016928,"PA 80A510","+","+","+",8034627,19,2001]
[null,5,"PA ..80A510 AS","-","+",1,8016929,"PA 80A510 AS","+","+","+",8034628,19,2001]
[null,6,"PA ..80A520","+","-",1,8016930,"PA 80A520","+","+","+",8034630,19,2001]
[null,7,"PA ..80A520 AS","+","+",1,8016931,"PA 80A520 AS","+","+","+",8034632,19,2001]
[null,8,"PA ..80B421","+","+",2,8016939,"PA 80B421","+","+","+",8034633,19,2001]
[null,9,"PA ..10B421","+","+",2,8016941,"PA 10B421","+","+","+",8034635,21.5,2001]
[]
[]
[null,null,null,"Uwagi:"]
[null,null,null,"Wkładka do IO - WKP 518, SAP - 8034753"]
[null,null,null,"Częsć wewnętrzna pokrętła PAS - SAP 8024397"]
[null,null,null,"Podpora płytki serwisowej PAS - SAP 8024396"]
[]
[null,null,null,"Wszystkie powyższe elementy są pakowane do jednego pudełka łacznie ze sterownikiem."]

{"sheet":"Tabele pomocnicze","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}