{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":64,"n_cols":4,"rows_kept":64,"cut":false,"hidden":false,"merged":[[21,2,21,3],[24,2,24,3],[31,2,31,3],[51,2,51,3],[56,2,56,3],[60,2,60,3],[35,2,35,3],[40,2,40,3],[46,2,46,3]],"flags":["formulas_cached_only"]}
[]
["Sada č.1 ( 4 kusy ) ","Počet kusů","FS cookers"]
["8023666 - Injector BSI-68526 UM 508 ( G30/36 - 0,52 )",1,"G5E3.32ZpTaKDSpNVm"]
["8023667 - Injector BSI-68524 UM 404 ( G30/36 - 0,67 )",2,"G5E3.32ZpTaVm"]
["8023668 - Injector BSI-68525 UM 404 ( G30/36 - 0,85 )",1,"G5E3.32ZpVm"]
[null,null,"G5E3.42ZpTaRSpNVm"]
[null,null,"G5E3.42ZpTaVm"]
[null,null,"G5E3.42ZpVm"]
[null,null,"G5E3.43ZpDVm"]
[null,null,"G5E3.43ZpTaKDRSpNVm"]
[]
["Sada č.2 ( 4 kusy ) ","Počet kusů","FS cookers"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",2,"G5E3.43ZpTkKDpRSpN"]
["8005519 - Injector drg. 0222/ 0,52",1,"G5E3.43ZpTkKDpSpN"]
["8000262 - Injector drg. 0222/ 0,80",1,"G5G4.42ZpMSpVm"]
[null,null,"G6E3.32S2ZpTe"]
[null,null,"G6E3.32S2ZpTeWsb"]
[null,null,"CEE3.400..."]
[null,null,"G6E3.33S2ZpTeKDWsb"]
[null,null,"G6E3.43S2ZpTeKDSp"]
[]
["Sada č.3 ( 4 kusy )","Počet kusů","BI GAS COOKERS"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",2,"EGH3.43ZpTeOKDW","GH 0503"]
["8005519 - Injector drg. 0222/ 0,52",1,"EGH3.43ZpTeOKDSr","GH 0103"]
["8000262 - Injector drg. 0222/ 0,80",1,"BI GAS HOBS 60cm"]
[null,null,"PSG4.0ZpZtR","PG 1920"]
[null,null,"PSG4.0ZpZtW","PG 2120"]
[null,null,"PMG4.0ZpZtCRetro","PG 1520"]
[null,null,"PSG4.0ZpW","PG 1820"]
[null,null,"PSG4.0ZpR","PG 1620"]
[]
["Sada č.4 ( 2 kusy )","Počet kusů","BI GAS HOBS 30cm"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",1,"PMG2.0ZpZt","PG 0920"]
["8005519 - Injector drg. 0222/ 0,52",1,"PMG2.0ZpZtR","PG 0720"]
[]
["Sada č.5 ( 5 kusů )","Počet kusů","BI GAS HOBS 79cm with \"FISCH\" burner"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",3,"PSG5.1ZpZtR","PG 2520"]
["8005519 - Injector drg. 0222/ 0,52",1,"PSG5.1ZpZtR","PG 2525"]
["8000262 - Injector drg. 0222/ 0,80",1]
[]
["Sada č.6 ( 5 kusů )","Počet kusů","BI GAS HOBS 79cm with \"WOK\" burner"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",2,"PSG5.0ZpZtR","PG 2220"]
["8005519 - Injector drg. 0222/ 0,52",1,"PSG5.0ZpZtR","PG 2225"]
["8000262 - Injector drg. 0222/ 0,80",1]
["8000461 - Injector drg. 0222/ 0,95",1]
[]
["Sada č.7 ( 4 kusy )","Počet kusů","BI GAS HOBS 60cm with \"WOK\" burner"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",2,"PSG4.1ZpZtR","PG 1921"]
["8005519 - Injector drg. 0222/ 0,52",1]
["8000461 - Injector drg. 0222/ 0,95",1]
[]
["Sada č.8 ( 3 kusy )","Počet kusů","BI COMBINATION HOBS 60cm"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",1,"PSG3.1ZpZtR","PG 2820"]
["8005519 - Injector drg. 0222/ 0,52",1]
["8000262 - Injector drg. 0222/ 0,80",1]
[]
["Sada č.9 ( 2 kusy )","Počet kusů","BI COMBINATION HOBS 60cm"]
["8005519 - Injector drg. 0222/ 0,52",1,"PCG2.2ZpZtR","GC 0220"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",1]
[]
["Sada č.10 ( 3 kusy )","Počet kusů","BI COMBINATION HOBS 60cm"]
["8000461 - Injector drg. 0222/ 0,95",1,"PSG5.2ZpZtR","PG 2125"]
["8000354 - Injector drg. 0222/ 0,65 S1, S2 - 28-30mbar",1]
["8005519 - Injector drg. 0222/ 0,52",1]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}